Sep 28 1999 11:04 Page �

UDP_header.txt

                   0      7 8     15 16    23 24    31
                  +--------+--------+--------+--------+
                  |     Source      |   Destination   |
                  |      Port       |      Port       |
                  +--------+--------+--------+--------+
                  |                 |                 |
                  |     Length      |    Checksum     |
                  +--------+--------+--------+--------+
                  |
                  |          data octets ...
                  +---------------- ...

                       User Datagram Header Format

 Fields
 ------

 Source Port is an optional field, when meaningful, it indicates the port
 of the sending  process,  and may be assumed  to be the port  to which a
 reply should  be addressed  in the absence of any other information.  If
 not used, a value of zero is inserted.

 Destination  Port has a meaning  within  the  context  of  a  particular
 internet destination address.

 Length  is the length  in octets  of this user datagram  including  this
 header  and the data.   (This  means  the minimum value of the length is
 eight.)

 Checksum is the 16-bit one’s complement of the one’s complement sum of a
 pseudo header of information from the IP header, the UDP header, and the
 data,  padded  with zero octets  at the end (if  necessary)  to  make  a
 multiple of two octets.

 The pseudo  header  conceptually prefixed to the UDP header contains the
 source  address,  the destination  address,  the protocol,  and the  UDP
 length.   This information gives protection against misrouted datagrams.
 This checksum procedure is the same as is used in TCP.

                   0      7 8     15 16    23 24    31
                  +--------+--------+--------+--------+
                  |          source address           |
                  +--------+--------+--------+--------+
                  |        destination address        |
                  +--------+--------+--------+--------+
                  |  zero  |protocol|   UDP length    |
                  +--------+--------+--------+--------+

Printed by toke from dtoke